Roland DGA Firmware Updater Application
User Instructions 1/2006 

1. Turn the main power of the unit on. (This power switch will be located near the power cord.) 

2. Hold down the up, left and down arrow keys while pressing the sub power button to enter the Firmware Upgrade mode. (The sub power button is found on the front panel of the printer.) 

3. The printer will display “version up are you sure”; press the “enter” key. 

4. The display will then read “waiting” indicating it is ready to receive firmware. 

5. Launch the “Roland Firmware Upgrader.exe” application. 

6. Enter the units TCP/IP address and then click “Next”. If this is a SP-300 or SP-300V unit, select SP-300 in the menu next to the option to “Output though a Windows Driver”. 

7. Click “Next” 

8. Click “Yes” 

9. The Roland Firmware Updater Application will start to transfer the firmware to the unit. 

10. Click “Finish” to close the application. 

11. The Roland unit’s display will show “erasing” then “writing” and then “complete”. 

12. Once the display reads “complete” you may then power down the unit and restart it. 

13. Make sure when the printer powers back up to check the firmware version to confirm that it was completely installed. 

14. You have now completed the firmware upgrade.

**If problems arise during firmware updating or if you have any questions on this procedure, please contact your local Roland DGA Authorized Reseller or Roland DGA Technical Support (800-542-2307). Thank you
