[Cut Setting] dialog box

Use cutting conditions of machine
This uses the cutting conditions set for the connected cutting machine.
When disabled, the following conditions can be set.

- Cut Force: This sets the force for cutting.
- Cut Speed: This sets the speed at which the cutting carriage moves when cutting.
- Cutter Offset: This sets the offset amount from the center of the holder to the edge of the cutter.
- Cutter Length: This sets the length of the portion to cut with perforated cutting.
- Half Cut Length: This sets the length of the uncut portion with perforated cutting.
- Half Cut Force: This sets the force to apply to the uncut portion with perforated cutting.

Overlap Cutting
Select "Machine settings" to apply the overlap cutting count set for the connected cutting machine.
This setting takes precedence when selecting values.

Cut Quality
Select "Machine settings" to apply the cut quality set for the connected cutting machine.
This setting takes precedence when selecting [HI-SPEED] or [NORMAL].