[Crop-marks] dialog box

Type
This selects the layout for crop marks.
Choose the name of the model you're using.
Choosing the SV-15/12/8 turns off the feature for printing crop marks.
(The SV-15/12/8 provides no feature for alignment using crop marks.)

Point
Select the number of crop marks to place.
Depending on your model, this option may be disabled.

W, L
These specify the positional relationship for the three marks.
Take into account the margins required when performing cutting and print the crop marks inside these margins.
For more information, see "Crop Marks."

X, Y
Here you enter the location of the mark at the lower left.
Take into account the margins required when performing cutting and print the crop marks inside these margins.
For more information, see "Crop Marks."